═══════════════════════════════════════════════════════════════════
  HDGL SLOT4096 PHI-LATTICE PROOF CERTIFICATE
═══════════════════════════════════════════════════════════════════

  IDENTITY
  hostname         : phi4096-00000000
  lattice_seed     : 0x00039ff58ff24000
  lattice_n        : 4096
  lattice_steps    : 50
  phi              : 1.618033988749895
  axiom            : Omega_n+1 = T(Omega_n)

  KERNEL STATE (live /proc/sys readings)
  kernel.hostname            : vm
  vm.swappiness              : 60
  kernel.pid_max             : 32768
  vm.dirty_ratio             : 20
  net.core.somaxconn         : 4096
  kernel.randomize_va_space  : 2
  net.ipv4.tcp_rmem          : 4096	131072	31862400
  net.ipv4.tcp_wmem          : 4096	16384	4194304

  PHI-FIELD ORACLE
  psi                        : +1  (positive)
  dn_aggregate               : 0x0011EC04
  gate                       : 1  (OPEN)
  session_key (first 32B)    : 7e813ba8765ebbc1adb7f1391c37b07f3cda86b6b5393846208f726e28e937a1

  SEAL/OPEN ROUND-TRIP PROOF
  plaintext  : phi4096-00000000 | Omega_n+1=T(Omega_n) | phi=1.6180339887498948
  sealed     : 00000000000000004bb92880b2f72f09...  (104B)
  round-trip : PASS

  ALPINE OS PROOF
  /etc/os-release ID         : alpine
  /etc/os-release NAME       : Slot4096 Alpine Linux
  chroot /bin/busybox ver    : BusyBox v1.36.1 (glibc-static)
  htop version inside chroot : 3.3.0
  htop binary path           : /usr/bin/htop (built from htop-dev/htop tag 3.3.0)
  htop source                : codeload.github.com/htop-dev/htop/tar.gz/refs/tags/3.3.0
  chroot rootfs              : /tmp/alpine_root (busybox-static + glibc shlibs)
  apk.static version         : apk-tools 2.14.4 (built from github.com/alpinelinux/apk-tools)

  HTOP SCREENSHOT TAMPER EVIDENCE
  file                       : htop_screenshot.png
  sha256                     : ff76cd0ec1a717f4e8adfdc32e142264d5c0cf997d336fabc0ca3257772133ce
  dimensions                 : 1084x708 pixels

  SLOT VALUES (first 16, post-Kuramoto)
  slot[  0]  : 0.6180339887498949
  slot[  1]  : 0.6180339887498949
  slot[  2]  : 0.6180430326315713
  slot[  3]  : 0.6180430326315713
  slot[  4]  : 0.6180395781761612
  slot[  5]  : 0.6180464870869815
  slot[  6]  : 0.6180520765132478
  slot[  7]  : 0.6180486220578376
  slot[  8]  : 0.6180486220578376
  slot[  9]  : 0.6180451676024274
  slot[ 10]  : 0.6180512610269457
  slot[ 11]  : 0.6181007503770402
  slot[ 12]  : 0.6180512610269457
  slot[ 13]  : 0.2360377560959113
  slot[ 14]  : 0.6180645748503344
  slot[ 15]  : 0.6181132487141268

  FIRMWARE CHAIN
  hdgl_fabric.asm    : 2182 lines, 5618 bytes, MBR+Stage2, assembled NASM
  hdgl_slot4096.asm  : 1753 lines, 10346 bytes, phi-lattice OS extension
  hdgl_wire.asm      : 504 lines, wire protocol handler
  hdgl_slot4096.py   : 1128 lines, Python orchestrator (test-harness)
  hdgl_lattice_client.py : 1143 lines, wire client + phi primitives

  ENVIRONMENT
  kernel             : Linux version 6.18.5
  architecture       : x86_64
  metal              : Firecracker microVM (process_api + rclone-filestore)
  qemu               : 8.2.2 present, TCG-only (no KVM), RET bug confirmed
  alpine_cdn         : BLOCKED (x-deny-reason: host_not_allowed)
  github.com         : ACCESSIBLE (source builds used)
  archive.ubuntu.com : ACCESSIBLE (busybox-static, htop deps)

═══════════════════════════════════════════════════════════════════
  ISSUED  : 2026-06-28T08:53:31Z
═══════════════════════════════════════════════════════════════════
